How to operate ESP32:

First download the CP210x drivers that fit your device

After downloading the CP210x, you will enter the program and connect the ESP32

Download the latest version of the Arduino program to programming the code

Download Link:

www.arduino.cc/en/sftware

After that download the upgraded version of ARDUINO-ESP32 and then write the required codes and then we can use the widget